Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## micromod.output
Interface PCM16

All Known Implementing Classes:
  PCM16StreamOutputDevice

public interface PCM16

PCM (Pulse Code Modulation) audio consists of regularly spaced "impulses". The spacing of these impulses per second is determined by the sampling rate. A correct implementation of this interface should contain an appropriate representation of 16 bit PCM audio.

Method Summary
`int` | `getSamplingRate()`

Method Detail

### getSamplingRate

    public int getSamplingRate()

  Returns:
    The PCM sampling rate

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD